Note: Please send data as in below listed sheet or any other forms to our email: info@fountom.com

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Client Name | | *Fountom Marine* | | | Destination Country | | *China* | | |
| Contact Email | | *info@fountom.com* | | | Delivery Terms | | *FOB Shanghai* | | |
| **No.** | **Product Name** | | | **Nominal Size** | **Specification/Type** | | **Material** | **Press. Rating** | **QTY** |
|
| Valves and Armatures | | | | | | | | | |
| 1 | Air Vent | | | DN100 | | (With flame arrestor) |  | PN10 | 1 |
| 2 | SDNR Valve | | | DN50 | | Flanged Type | CI | PN10 | 3 |
| 3 | Buttterfly Valve | | | DN200 | | Flanged Type | CI | PN10 | 2 |
| 4 | Globe Valve | | | DN32 | | Flanged Type | CI | PN10 | 12 |
| 5 | Non Return Valve | | | DN25 | | Flanged, Thread type | CI | PN10 | 1 |
| 6 | Strainer | | | DN65 | | Mesh Size 5mm, flanged Type | CI | PN10 | 1 |
| 7 | Mud box | | | DN65 | | Flanged Type | CI | PN10 | 3 |
| 8 | Fire Hydrant | | | DN50 | | Flanged,angle Type | Brass | PN10 | 5 |
| 9 | Bilge Ejector | | | DN50/50/80 | | [20m](mailto:20m3/h@30MWC)[3](mailto:20m3/h@30MWC)[/h@30MWC](mailto:20m3/h@30MWC) | CI | PN10 | 1 |
| 10 | Quick closing Valve | | | DN40 | | Flanged,Mechanical Type | Ductile Cast Iron | PN10 | 1 |
| 11 | Check Valve | | | DN32 | | Swing check Type | CI | PN10 | 1 |
| 12 | Simplex Filter | | | DN50 | | Mesh Size 300 micron ,flanged Type | CI | PN10 | 1 |
| 13 | Gate Valve | | | DN100 | | Flanged Type | CI | PN10 | 3 |
| 14 | Self closing Drain Valve | | | DN20 | | Flanged Type | CI | PN10 | 5 |
| 15 | Safety Relief Valve | | | DN100 | | Flanged Type | CI | PN10 | 2 |
| 16 | Duplex LO Filter | | | DN100 | | Mesh Size 50micron ,flanged Type | CI | PN10 | 2 |
| 17 | Compensator/Bellows | | | DN500 | | Flanged Type |  | PN10 | 4 |
| 18 | High Temp Ball Valve | | | DN25 | | With Female Thread (Temperature 500°C) |  | PN10 | 5 |
| 19 | Swing type Non Return Valve | | | DN10 | | thread type | CI | PN10 | 2 |
| 20 | Pressure Relief Valve | | | DN25 | | Set Pressure 8bar |  | PN16 | 1 |
| 21 | Y- Type Strainer | | | DN15 | | Mesh Size 0.1 mm | CI | PN16 | 1 |
| 22 | Bilge Ejector | | | DN80/100 | | 45m3/35mwc |  | PN40 | 2 |
| 23 | Pressure Gauge (Dial Type) | | | 1/4" | | (0 to 10)bar | SS |  | 16 |
| 24 | Gauge Cock | | | 1/4" | |  | Brass |  | 35 |
| 25 | Temparature Indicator | | | 1/2" | | 120deg | SS |  | 10 |
| 26 | Flushing cap with Inner Thread Socket | | | DN 40 | |  | Brass |  | 12 |
| 27 | Sounding cap with chain | | | DN 40 | |  | Brass |  | 6 |
| 28 | Fire Hydrant | | | DN50 | | Flanged,angle Type, storz coupling | Brass | PN10 | 6 |
| 29 | Pressure Reducting Valve | | | DN25 | | 30bar-7bar | Brass | PN40 | 1 |
| 30 | Pressure Relief Valve | | | DN25 | | Set Pressure 8bar |  | PN40 | 1 |
| 31 | swing Check Valve | | | DN25 | |  | CI | PN10 | 1 |
| 32 | Self Closing Sounding cock | | | DN40 | | (with small dia self closing cock) | Brass | PN10 | 9 |
| 33 | Mud box | | | DN80 | | Flangd straight Type | CI | PN10 | 1 |
| 34 | Duplex Fuel Filter | | | DN40 | | Mesh Size100micron ,flanged Type | CI | PN10 | 2 |
| 35 | Y- Type Strainer | | | DN15 | | Mesh Size 0.1 mm | CI | PN10 | 1 |
| 36 | MAGNETIC LEVEL GAUGE | | |  | | Measure Height 1000mm-4800mm |  |  | 10 |
| Remark | | |  | | | | | | |
| Expected Delivery Date | | | 05/31/2019 | | | Max Pack Per Unit | Tons | | |